DECK PANEL ADJUSTMENT

id091600810100

1. Loosen the installation nuts for deck panel.

e5e916zw6032

2. Adjust the gap and height difference between the deck panel and trunk lid within the specification by moving the deck panel back and forth, left and right, and by adjusting the number of shims if necessary.

e5e916zw6031

  Clearance

  a:4—6 mm {0.16—0.23 in}
  b:-2—2 mm {-0.07—0.07 in}

3. Tighten the nuts.