PLANETARY GEAR COMPONENT INSPECTION

id051300261300

1. Using a dial gauge, measure the inner diameter of the front planetary ring gear flange bushings.

bsj6za00000288

  Front planetary ring gear bushing inner diameter

  46.038—46.063 mm {1.81252—1.81350 in}

  Caution
  • Measure at different places and take an average. If it exceeds the specification, replace the front planetary ring gear flange with a new one.
  • When the front planetary ring gear flange is replaced, inspect the contact surface opposed to the middle planetary gear component.
  • If the surface of it is scratched or has changed color, replace the middle planetary gear component with a new one.

2. Using a dial gauge, measure the inner diameter of the front planetary gear component bushings.

bsj6za00000289

  Front planetary gear component bushing inner diameter

  48.755—48.780 mm {1.91949—1.92047 in}

  Caution
  • Measure at different places and take an average. If it exceeds the specification, replace the front planetary gear component with a new one.
  • When the front planetary gear component is replaced, inspect the contact surface opposed to the clutch hub.
  • If the surface of it is scratched or has changed color, replace the clutch hub with a new one.

3. Using a dial gauge, measure the inner diameter of the rear planetary gear component bushings.

bsj6za00000849

  Rear planetary gear component bushing inner diameter

  18.000—18.025 mm {0.7087—0.7096 in}

  Caution
  • Measure at different places and take an average. If it exceeds the specification, replace the rear planetary gear component with a new one.
  • When the rear planetary gear component is replaced, inspect the contact surface opposed to the intermediate shaft.
  • If the surface of it is scratched or has changed color, replace the intermediate shaft with a new one.