POWER RETRACTABLE HARDTOP DRAIN HOSE REMOVAL/INSTALLATION

id091600821300

1. Fully close the power retractable hardtop.

2. Fully open the deck panel.

3. Remove clip A, and remove the power retractable hardtop drain hose from the rear window glass.

e5e916zw6066

4. Insert your hand from the fully opened deck panel and remove clip B, and remove the power retractable hardtop drain hose from the rear side trim.

5. Install in the reverse order of removal.