TRANSMISSION/TRANSAXLE TECHNICAL DATA

id055000800100

Clutch

Item | Specification
--- | ---
Clutch fluid | European (L.H.D. U.K.) specs.: SAE J1703, FMVSS 116 DOT-3 or DOT-4 Australian specs.: SAE J1703, FMVSS 116 DOT-3
Clutch pedal stroke | L.H.D.: 130 mm {5.12 in} R.H.D.: 131.6 mm {5.181 in}
Clutch pedal play | 5—15 mm {0.20—0.59 in}
Clutch pedal push rod play | At push rod setting line: 0.1—0.5 mm {0.004—0.020 in} (Reference value) At pedal pad: 0.5—2.7 mm {0.020—0.106 in}
Clutch disengagement stroke (Reference value) | A: 80—110 mm {3.15—4.33 in}
Clutch disc maximum depth | 0.6 mm {0.024 in}
Clutch cover maximum clearance | 0.5 mm {0.020 in}
Clutch cover maximum height difference | 1.0 mm {0.039 in}
Clutch disc minimum depth | 0.3 mm {0.012 in}
Clutch disc maximum runout | 0.7 mm {0.028 in}
Flywheel maximum runout | 0.1 mm {0.004 in}

Manual Transmission [M15M-D]

Item | Specification
--- | ---
Specified oil grade | API Service GL-4 or GL-5
Specified oil viscosity | All season: SAE 75W-90 Above 10°C {50°F}: SAE 80W-90
Capacity (approx. quantity) | 2.0 L {2.1 US qt, 1.8 lmp qt}
Shift control case specified oil grade | API Service GL-4 or GL-5
Shift control case specified oil viscosity | SAE 75W-90
Shift control case capacity (approx. quantity) | 290—330 ml {290—330 cc, 17.69—20.13 cu in}

Manual Transmission [P66M-D]

Item | Specification
--- | ---
Transmission case specified oil grade | API Service GL-4
Transmission case specified oil viscosity | SAE 75W-90
Transmission case capacity (approx. quantity) | 2.1 L {2.2 US qt, 1.8 lmp qt}
Shift control case specified oil grade | API Service GL-4
Shift control case specified oil viscosity | SAE 75W-90
Shift control case capacity (approx. quantity) | 80—230 ml {80—230 cc, 4.88—14.03 cu in}

Automatic Transmission [SJ6A-EL]

Item | Specification
--- | ---
Time lag | N position → D range: 0.7 s or less N position → R position: 1.2 s or less
ATF | Type: JWS3309 Capacity (approx. quantity): 7.4 L {7.8 US qt, 6.5 lmp qt}
Turbine sensor resistance | 560—680 ohm
VSS resistance | 560—680 ohm
Distance A between end of torque converter and face of converter housing | 26.2 mm {1.03 in}

Line pressure

Position/Range | Specification (kPa {kgf/cm2, psi})
--- | ---
D, M | Idle | 355—425 {3.7—4.3, 52—61}
Stall | 863—959 {8.8—9.7, 126—139}
R | Idle | 804—942 {8.2—9.6, 117—136}
Stall | 1,424—1,608 {14.6—16.3, 207—233}

Engine stall speed

Position/Range | Specification (rpm)
--- | ---
D, R, M | 2,307—2,607

Transmission fluid temperature (TFT) sensor

ATF temperature (°C {°F}) | Resistance (kilohm)
--- | ---
10 {50} | 6.445
25 {77} | 3.5
110 {230} | 0.247

Solenoid valve resistance (ATF temperature: 20 °C {68 °F})

Terminals | Solenoid valve | Resistance (ohm)
--- | --- | ---
O—GND | Shift solenoid A | 5.0—5.6
N—GND | Shift solenoid B | 5.0—5.6
M—GND | Shift solenoid C | 5.0—5.6
L—GND | Shift solenoid D | 5.0—5.6
K—GND | Shift solenoid E | 5.0—5.6
E—F | Shift solenoid F | 5.0—5.6
C—D | Shift solenoid G | 5.0—5.6
I—J | Line pressure control solenoid | 5.0—5.6
G—H | TCC control solenoid | 5.0—5.6