FUEL INJECTOR INSPECTION [L8, LF]

id0114a3800700

Resistance Inspection

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the fuel injector connector.

4. Inspect the resistance between fuel injector terminals A and B.

amxzzw00000905

  • If not within the specification, replace the fuel injector. (See FUEL INJECTOR REMOVAL/INSTALLATION [L8, LF].)

  Fuel injector resistance

  11.4—12.6 ohms [20 °C {68 °F}]