HEADLIGHT CLEANER MOTOR REMOVAL/INSTALLATION

id091900803300

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the washer tank. (See WASHER TANK REMOVAL/INSTALLATION.)

4. Remove the bolt, then remove the bracket.

amxzzw00000737

5. Remove the headlight cleaner motor, then remove the grommet.

6. Install in the reverse order of removal.