FRONT FENDER PANEL REMOVAL/INSTALLATION

id091000405900

1. Disconnect the negative battery cable. (SeeBATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Remove the side step molding. (SeeSIDE STEP MOLDING REMOVAL.) (SeeSIDE STEP MOLDING INSTALLATION.)

5. Remove in the order indicated in the table.

e5u910zw1023

1 | Fastener
2 | Bolt A
3 | Bolt B
4 | Bolt C
5 | Bolt D
6 | Front fender panel

6. Install in the reverse order of removal.