CYLINDER BLOCK INSPECTION

id011000507200

1. Measure the distortion of the cylinder block top surface in six directions as indicated in the figure.

  • If it exceeds the maximum, replace the cylinder block.

belbze00000102

  Maximum cylinder block distortion

  0.10 mm {0.004 in}

2. Measure the cylinder bores in X and Y directions at 42 mm {1.65 in} below the top surface.

  • If not within the specification, replace the cylinder block.

belbze00000103

  Standard cylinder bore diameter

  L8: 82.940—83.090 mm {3.2653—3.2712 in}
  LF, L3: 87.440—87.590 mm {3.4425—3.4484 in}
  L5: 88.940—89.090 mm {3.5016—3.5074 in}