PASSENGER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION

id081000801900

  Warning
  • Handling the air bag module improperly can accidentally deploy the air bag module, which may seriously injure you. Read the service warnings and cautions before handling the air bag module. (See AIR BAG SYSTEM SERVICE WARNINGS.) (See AIR BAG SYSTEM SERVICE CAUTIONS.)
  • If the passenger-side air bag module is installed with debris in the module, it may be scattered when the air bag module operates (deploys), causing injury. Verify that there is no debris in the passenger-side air bag module before installation.
  • If a damaged passenger-side air bag module is installed, the vehicle may be damaged or the passenger may be injured when the air bag module operates (deploys). Verify that the passenger-side air bag has no damage before installation.

1. Turn the ignition switch to the LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable and wait for 1 min or more. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

5. Remove the cap. (See Cap Installation Note.)

amxzzw00001834

6. Using a flathead screwdriver, lift the locking device carefully, however do not remove it.

7. Disconnect the connector.

8. Remove the screw A.

9. Remove the nuts.

10. Remove the brackets.

11. Remove the screw B.

12. Remove the passenger-side air bag module in the order indicated below.

  (1) Disengage the tab locks by sliding the passenger-side air bag module upward.

  amxzzw00001835

  (2) Slide the passenger-side air bag module rearward.

  (3) Remove the passenger-side air bag module by pulling it from the backside and then down.

13. Install in the reserve order of removal.

14. Turn the ignition switch to the ON position.

15. Verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system. (See FLOWCHART [AIR BAG SYSTEM].)

Cap Installation Note

1. The cap cannot be reused. Replace the cap with a new one when the cap or the passenger-side air bag module has been removed.