INSTRUMENT CLUSTER STRUCTURAL VIEW

id092200531300

Meter And Gauge

amxzzn00000631

Warning And Indicator Light

amxzzn00000723

×: Applicable

No. | Warning and indicator light | Input signal source | CAN system | Description | Note
--- | --- | --- | --- | --- | ---
1 | MIL | PCM | × | Illuminates if a malfunction occurs in the engine control system and the automatic transmission control system. (See ON-BOARD DIAGNOSTIC SYSTEM MALFUNCTION DISPLAY FUNCTION [L8, LF].) | —
2 | ABS warning light | • DSC HU/CM • ABS HU/CM | × | If the ABS/DSC system is malfunctioning, the ABS warning light remains illuminated. | —
3 | DSC OFF light | DSC HU/CM | × | • If the DSC system is malfunctioning, the DSC OFF light remains flashed. • When the DSC OFF switch is pressed to disable, the DSC OFF light illuminates. | With DSC
4 | DSC indicator light | DSC HU/CM | × | • If the DSC system is malfunctioning, the DSC indicator light remains illuminated. • When the DSC or TCS is operating, the DSC indicator light flashes. | With DSC
5 | Turn indicator light | Flasher control module | — | • Flashes when ignition switch is ON position during turn switch operation. • Flashes when hazard switch is on. | —
6 | High-beam indicator light | Instrument cluster (Light switch (HI)) | — | When the headlight (high-beam) illuminates, the high-beam indicator light illuminates. | —
7 | Security light | Keyless control module | × | Illuminates or flashes when immobilizer system has malfunction. | —
8 | Front fog indicator light | Instrument cluster (Front fog light relay) | — | When the front fog light illuminates, the front fog indicator light illuminates. | With front fog light
9 | Rear fog indicator light | Instrument cluster (Rear fog light relay) | — | When the rear fog light illuminates, the rear fog light indicator light illuminates. | With rear fog light
10 | Headlight auto leveling warning light | Auto leveling control module | — | The headlight auto leveling system warning light illuminates if a malfunction in the auto leveling system is detected. | With headlight auto leveling system
11 | Cruise main indicator light | PCM | × | Illuminates if the cruise control system is in control status. (See CRUISE CONTROL SYSTEM OUTLINE [L8, LF].) | With cruise control system
Cruise set indicator light
12 | Brake system warning light | PCM | × | Brake system warning light. illumination request (See DRIVE-BY-WIRE CONTROL OPERATION [L8, LF].) | —
• DSC HU/CM • ABS HU/CM | × | If the ABS/DSC system is malfunctioning, the brake system warning light remains illuminated. | —
• Instrument cluster (Parking brake switch) • Instrument cluster (Brake fluid level sensor) | — | • When the parking brake is operating, the brake system warning light illuminates. • When the brake fluid-level is low, the brake system warning light illuminates. | —
13 | Door ajar warning light | Instrument cluster (Door switches) | — | Illuminates when door or trunk lid is open. | —
14 | Seat belt warning light | Instrument cluster (Buckle switch) | — | When the driver’s seat belt is not fastened, the seat belt warning light illuminates. | —
15 | Air bag system warning light | SAS control module | — | Illuminates or flashes when SRS air bag system has malfunction. | —
16 | Malfunction warning light | PCM | × | Malfunction warning light illumination request. (See DRIVE-BY-WIRE CONTROL OPERATION [L8, LF].) | With malfunction warning light
17 | AT warning light | TCM | × | The AT warning light illuminates to alert the driver of a malfunction in the automatic transmission. (See AT WARNING LIGHT FUNCTION [SJ6A-EL].) | AT
Gear shift indicator | PCM | × | Gear shift indicator illumination request. (See GEAR SHIFT INDICATOR OPERATION [L8, LF].) | With gear shift indicator
18 | Active bonnet warning light | Active bonnet control module | × | If the active bonnet system is malfunctioning, the active bonnet warning light remains illuminated. (See ACTIVE BONNET WARNING ALARM CONSTRUCTION/OPERATION.) | With active bonnet system
19 | Gear position indicator light | TCM | × | The gear position indicator light displays the gear position when in the manual mode. (See SELECTOR INDICATOR LIGHT FUNCTION [SJ6A-EL].) | AT
20 | Selector indicator light | TCM | × | The selector indicator light displays the selector lever position. (See SELECTOR INDICATOR LIGHT FUNCTION [SJ6A-EL].) | AT
21 | Tire pressure monitoring system (TPMS) warning light | DSC HU/CM | × | If the TPMS system is malfunctioning or the tire pressure is abnormal, the TPMS warning light remains illuminated. | With TPMS
Malfunction warning light | PCM | × | Malfunction warning light illumination request. (See DRIVE-BY-WIRE CONTROL OPERATION [L8, LF].) | With malfunction warning light
22 | Generator warning light | PCM | × | Illuminates if the generator output is not normal. (See GENERATOR CONSTRUCTION [L8, LF].) | —
23 | Fuel-level warning light | Instrument cluster (Fuel gauge sender unit) | — | When the remaining fuel amount in the fuel tank is low, the fuel-level warning light illuminates. | —