VARIABLE TUMBLE SOLENOID VALVE INSPECTION [L8, LF]

id0113a3802900

Airflow Inspection

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the variable tumble solenoid valve. (See VARIABLE TUMBLE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].)

4. Inspect airflow between the ports under the following conditions.

amxzzw00000901

amxzzw00000803

  • If not as specified, replace the variable tumble solenoid valve. (See VARIABLE TUMBLE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].)