POWER RETRACTABLE HARDTOP OPEN/CLOSE WARNING BEEP ON/OFF SWITCHING

id091600812100

1. Connect the M-MDS to the DLC-2.

e5e916zw6082

2. After the vehicle is identified, select the following items from the initial screen of the M-MDS.

  • When using the IDS (laptop PC)
  1.Select”Module Programming”.
  • When using the PDS (Pocket PC)
  1.Select “Programming”.
  2.Select “Module programming”.

3. Then, select items from the screen menu in the following order.

  (1) Select “Programmable Parameters”.

  (2) Select “Warning Lamps/Chimes”.

4. Select the “following item” on the M-MDS to set Enabled/Disabled.

  Item

  • RHT Buzzer - (IC)