MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR INSPECTION [L8, LF]

id0140i7800900

1. Connect the M-MDS to the DLC‐2.

amxzzw00000039

2. Turn the ignition switch to the ON position (Engine off).

3. Select MAP PID on the M-MDS.

4. Verify that the MAP PID (pressure) and barometric pressure are practically equal.

  • If not as specified, replace the MAP sensor. (See MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR REMOVAL/INSTALLATION [L8, LF].)