REAR FOG LIGHT RELAY REMOVAL/INSTALLATION

id092100802600

  Note
  • Depending on the period of manufacture, the trunk lid opener relay and rear fog relay positions may be switched. When performing removal/installation and inspection, make determinations based on wiring color.
    ― Terminal A: blue/red
    ― Terminal C: light green
    ― Terminal D: red/blue
    ― Terminal E: black/green

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

4. Remove the rear fog light relay.

d5e921zw6002

5. Install in the reverse order of removal.