- QUICK DIAGNOSTIC CHART [INSTRUMENT CLUSTER]
- SYMPTOM TROUBLESHOOTING [INSTRUMENT CLUSTER]
- NO. 1 FUEL GAUGE NEEDLE POSITION INCORRECT [INSTRUMENT CLUSTER]
- NO. 2 ALL METERS AND GAUGES DO NOT OPERATE [INSTRUMENT CLUSTER]
- NO. 3 ABS WARNING LIGHT ILLUMINATES [INSTRUMENT CLUSTER]
- NO. 4 MIL ILLUMINATES [INSTRUMENT CLUSTER]
- NO. 5 BRAKE SYSTEM WARNING LIGHT ILLUMINATES [INSTRUMENT CLUSTER]
- NO. 6 INSTRUMENT CLUSTER ILLUMINATION DOES NOT ILLUMINATE [INSTRUMENT CLUSTER]
- NO. 7 SPEEDOMETER INDICATION IS DEFECTIVE [INSTRUMENT CLUSTER]
- NO. 8 TACHOMETER INDICATION IS DEFECTIVE [INSTRUMENT CLUSTER]
- NO. 9 WATER TEMPERATURE GAUGE INDICATION IS DEFECTIVE [INSTRUMENT CLUSTER]
- NO. 10 OIL PRESSURE GAUGE INDICATION IS DEFECTIVE (OIL PRESSURE GAUGE NEEDLE DOES NOT MOVE FROM THE L POSITION OR LESS) [INSTRUMENT CLUSTER]
- NO. 11 MALFUNCTION WARNING LIGHT ILLUMINATES [INSTRUMENT CLUSTER]