ON-BOARD DIAGNOSTIC SYSTEM PID/DATA MONITOR FUNCTION [ABS]

id0402a7181800

• The PID/data monitor function is used for optionally selecting input/output signal monitor items preset in the ABS HU/CM and reading them out in real-time.

PID/DATA Monitor Table

PID/data monitor item | Input/output part | Unit/Condition (Tester display)
--- | --- | ---
ABS_VOLT | Battery | V
ABSLF_I | LF inlet solenoid valve | Off/On
ABSLF_O | LF outlet solenoid valve | Off/On
ABSLR_I | LR inlet solenoid valve | Off/On
ABSLR_O | LR outlet solenoid valve | Off/On
ABSPMPRLY | Pump motor relay | Off/On
ABSRF_I | RF inlet solenoid valve | Off/On
ABSRF_O | RF outlet solenoid valve | Off/On
ABSRR_I | RR inlet solenoid valve | Off/On
ABSRR_O | RR outlet solenoid valve | Off/On
ABSVLVRLY | Valve control relay | Off/On
BOO_ABS | Brake switch | Off/On
CCNTABS | Number of continuous DTCs | —
LF_WSPD | LF ABS wheel-speed sensor | KPH, MPH
LR_WSPD | LR ABS wheel-speed sensor | KPH, MPH
PMP_MOTOR | Pump motor | Off/On
RF_WSPD | RF ABS wheel-speed sensor | KPH, MPH
RR_WSPD | RR ABS wheel-speed sensor | KPH, MPH