INSPECTION AFTER TRANSMISSION INSTALLATION [M15M-D]

id051110246800

  Note
  • Perform the following inspection only when the transmission has been overhauled.

1. Perform a road test and inspect the following items:

  (1) No abnormal noise in each shift position.

  (2) Smooth shift operation when shifting gears.

  (3) No gear slipout after shifting gears.

  (4) Back-up light switch operates correctly.