COOLING FAN MOTOR INSPECTION [L8, LF]

id0112b4801800

Part Inspection

1. Verify that the battery is fully charged. (See BATTERY INSPECTION [L8, LF].)

2. Install a tester and battery to the cooling fan motor connector (4 terminals) as shown in the figure.

amxzzw00001972

Cooling fan motor rotation speed | Connection terminal
--- | ---
Positive | Negative
High | A and C | B and D
Middle | C | B and D
Low | C | B

3. Verify that the cooling fan motor operates smoothly at the standard current.

  • If there is any malfunction, replace the applicable part.

  Cooling fan motor standard current [12 V]

  High: 9.0—12.0 A
  Middle: 6.4—9.4 A
  Low: 4.8—7.8 A