PURGE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF]

id0116a3804300

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

Except 6MT

amxzzw00000847

6MT

amxzzw00000848

1 | Connector
2 | Vacuum hose (to dynamic chamber) (See Vacuum Hose Installation Note.)
3 | Evaporative hose (to charcoal canister) (See Evaporative Hose Installation Note.)
4 | Purge solenoid valve
5 | Bracket

3. Install in the reverse order of removal.

Evaporative Hose Installation Note

1. Fit the evaporative hose onto the respective fittings, and install clamps as shown.

amxzzw00000849

  (1) Insert the evaporative hose securely to the nipple.

  (2) Inspect the evaporative hose for damage and deformation.

Vacuum Hose Installation Note

1. Fit the vacuum hose onto the respective fittings, and install clamps as shown.

amxzzw00000849

  (1) Insert the vacuum hose securely to the nipple.

  (2) Inspect the vacuum hose for damage and deformation.