OIL PRESSURE INSPECTION [L8, LF]

id0111c6800300

  Warning
  • Hot engines and engine oil can cause severe burns. Turn off the engine and wait until it and the engine oil have cooled.
  • A vehicle that is lifted but not securely supported on safety stands is dangerous. It can slip or fall, causing death or serious injury. Never work around or under a lifted vehicle if it is not securely supported on safety stands.
  • Continuous exposure to USED engine oil has caused skin cancer in laboratory mice. Protect your skin by washing with soap and water immediately after working with engine oil.

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable.

3. Remove the under guard. (LF MT) (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].) (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)

4. Remove the oil pressure switch.

  Note
  • This inspection can be performed using a combination of SSTs 49 0187 280A (oil pressure gauge) and 49 E019 001 (adapter), or using the following combination of the SSTs.
    ― 49 D019 908 (gauge), 49 D019 909 (hose), 49 D019 910 (adapter), 49 D019 911 (adapter), and 49 D019 914 (adapter)

    amxzzw00001950

5. Install the SSTs to the oil pressure switch installation hole using the following procedure.

  Using SSTs 49 0187 280A and 49 E019 001

  1. Install SST 49 E019 001 to the oil pressure switch installation hole.
  2. Install SST 49 0187 280A to the SST 49 E019 001.

  Using SSTs 49 D019 908, 49 D019 909, 49 D019 910, 49 D019 911 and 49 D019 914

  1. Assemble SSTs 49 D019 910 and 49 D019 914 outside of the engine compartment beforehand.
  2. Assemble SSTs 49 D019 908, 49 D019 909 and 49 D019 911 outside of the engine compartment beforehand.
  3. Install SST 49 D019 914 to the oil pressure switch installation hole.
  4. Install SST 49 D019 911 to the SST 49 D019 910.

6. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

7. Warm up the engine to normal operating temperature.

8. Run the engine at the specified speed, and note the gauge readings.

  • If not within the specification, inspect for the cause and repair or replace if necessary.

  Note
  • The oil pressure can vary with oil viscosity and temperature.

  Oil pressure (reference value) [oil temperature: 100 °C {212 °F}]

  L8: 234—521 kPa {2.39—5.31 kgf/cm2, 33.9—75.5 psi}[3,000 rpm]
  LF: 337—591 kPa {3.44—6.03 kgf/cm2, 49.0—85.8 psi}[3,000 rpm]

9. Stop the engine and wait until it is cool.

10. Disconnect the negative battery cable.

11. Remove the SSTs.

  Caution
  • Be sure that there is no sealant between 1.0—2.0 mm {0.04—0.07 in} from the end of the oil pressure switch to prevent a possible operation malfunction.

12. Apply silicone sealant to the oil pressure switch threads as shown in the figure.

amxzzw00001951

13. Install the oil pressure switch.

  Tightening torque

  12—18 N·m {1.3—1.8 kgf·m, 9—13 ft·lbf}

14. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

15. Install the battery cover.

16. Start the engine and confirm that there is no oil leakage.

  • If there is oil leakage, repair or replace the applicable part.

17. Install the under guard. (LF MT) (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].) (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)