IGNITION COIL REMOVAL/INSTALLATION [L8, LF]

id0118a3800200

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the plug hole plate. (See PLUG HOLE PLATE REMOVAL/INSTALLATION [L8, LF].)

4. Remove the front suspension tower bar (joint). (See FRONT SUSPENSION TOWER BAR REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

e5u118zw5002

1 | Connector
2 | Ignition coil