AIRFLOW MODE MAIN LINK REMOVAL/INSTALLATION

id071100801800

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the airflow mode actuator. (See AIRFLOW MODE ACTUATOR REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER].) (See AIRFLOW MODE ACTUATOR REMOVAL/INSTALLATION [MANUAL AIR CONDITIONER].)

4. Remove the airflow mode main link as shown in the figure.

e5u711zw5006

5. Install in the reverse order of removal.