DTC P2195 [L8, LF]

id0102b1812700

DTC P2195 | A/F sensor signal stuck lean
--- | ---
DETECTION CONDITION | • The PCM monitors the A/F sensor output current when the following conditions are met. If the average output is more than 1.2 for 25 s, the PCM determines that the A/F sensor signal remains lean. MONITORING CONDITIONS ― ECT: more than 70 °C {158 °F} ― Engine speed: 1,000—3,200 rpm ― MAF amount: 6—80 g/s {0.80—10.58 lb/min} ― Target A/F feedback system status: feedback control ― Output voltage from the HO2S: more than 0.2 V Diagnostic support note • This is an intermittent monitor (A/F sensor, HO2S). • The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM. • PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA (Mode 2/Mode 12) is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • A/F sensor heater malfunction • A/F sensor malfunction ― Exhaust system leakage ― A/F sensor deterioration • MAF sensor malfunction • Air suction in intake air system • Improper operation of fuel injector • Fuel supply system malfunction or improper fuel line malfunction ― Pressure regulator (built-in fuel pump unit) malfunction ― Clogged or restricted fuel filter (built-in fuel pump unit) ― Fuel leakage in fuel line between fuel distribution pipe and fuel pump • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA (MODE 12) AND DIAGNOSTIC MONITORING TEST RESULTS HAVE BEEN RECORDED • Have the FREEZE FRAME DATA (Mode 12) and DIAGNOSTIC MONITORING TEST RESULTS (A/F sensor, HO2S related) been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA (Mode 12) and DIAGNOSTIC MONITORING TEST RESULTS on repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY RELATED PENDING CODE AND STORED DTC • Turn the ignition switch off, then to the ON position (engine off). • Perform the Pending Trouble Code Access Procedure and DTC Reading Procedure. (See ON-BOARD DIAGNOSTIC TEST [L8, LF].) • Is the DTC P2177 or P2187 also present? | Yes | Go to the applicable DTC troubleshooting. (See DTC P2177 [L8, LF].) (See DTC P2187 [L8, LF].)
No | Go to the next step.
4 | IDENTIFY TRIGGER DTC FOR FREEZE FRAME DATA (MODE 2) • Perform the Freeze Frame PID Data Access Procedure. (See ON-BOARD DIAGNOSTIC TEST [L8, LF].) • Is the DTC P2195 on FREEZE FRAME DATA (Mode 2)? | Yes | Go to the next step.
No | Go to the DTC troubleshooting on FREEZE FRAME DATA (Mode 2). (See DTC TABLE [L8, LF].)
5 | INSPECT A/F SENSOR HEATER • Inspect the A/F sensor heater. (See AIR FUEL RATIO (A/F) SENSOR INSPECTION [L8, LF].) • Is there any malfunction? | Yes | Replace the A/F sensor, then go to Step 13. (See AIR FUEL RATIO (A/F) SENSOR REMOVAL/INSTALLATION [L8, LF].)
No | Go to the next step.
6 | INSPECT A/F SENSOR • Inspect the A/F sensor. (See AIR FUEL RATIO (A/F) SENSOR INSPECTION [L8, LF].) • Is there any malfunction? | Yes | Go to the next step.
No | Go to Step 8.
7 | INSPECT GAS LEAKAGE FROM EXHAUST SYSTEM • Visually inspect if there is any gas leakage is found between the exhaust manifold and A/F sensor. • Is there gas leakage? | Yes | Repair or replace the malfunctioning part according to the inspection results, then go to Step 13. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)
No | Replace the A/F sensor, then go to Step 13. (See AIR FUEL RATIO (A/F) SENSOR REMOVAL/INSTALLATION [L8, LF].)
8 | VERIFY CURRENT INPUT SIGNAL STATUS OF MAF SENSOR • Connect the M-MDS to the DLC-2. • Start the engine. • Perform the PID/DATA Monitor and Record Procedure and access the MAF PID. (See ON-BOARD DIAGNOSTIC TEST [L8, LF].) • Verify that the MAF PID changes quickly according to engine speed. • Is the PID normal? (See PCM INSPECTION [L8, LF].) | Yes | Go to Step 10.
No | Go to the next step.
9 | INSPECT FOR EXCESSIVE AIR SUCTION OF INTAKE AIR SYSTEM • Visually inspect for loosen, cracks or damages hoses on intake air system. Note • Engine speed may change when rust penetrating agent is sprayed on the air suction area. • Is there any malfunction? | Yes | Repair or replace the malfunctioning part according to the inspection results, then go to Step 13.
No | Replace the MAF/IAT sensor, then go to Step 13. (See MASS AIR FLOW (MAF)/INTAKE AIR TEMPERATURE (IAT) SENSOR REMOVAL/INSTALLATION [L8, LF].)
10 | INSPECT FUEL INJECTOR OPERATION • Perform the Fuel Injector Operation Inspection. (See ENGINE CONTROL SYSTEM OPERATION INSPECTION [L8, LF].) • Is there any malfunction? | Yes | Repair or replace the malfunctioning part according to the inspection results, then go to Step 13.
No | Go to the next step.
11 | INSPECT FUEL LINE PRESSURE • Turn the ignition switch off. • Inspect the fuel line pressure. (See FUEL LINE PRESSURE INSPECTION [L8, LF].) • Is the fuel line pressure normal? | Yes | Go to Step 13.
No | Go to the next step.
12 | INSPECT FUEL SYSTEM FOR FUEL LEAKAGE • Visually inspect the fuel leakage in the fuel system. • Is there fuel leakage? | Yes | Repair or replace the malfunctioning part according to the inspection results, then go to the next step.
No | Inspect the fuel filters for the foreign material or stain inside the fuel filter (low-pressure side). If foreign material or stain is found inside the fuel filter (low-pressure side): • Clean the fuel tank and fuel filter. If normal: • Replace the fuel pump unit. (See FUEL PUMP UNIT REMOVAL/INSTALLATION [L8, LF].) Go to the next step.
13 | VERIFY DTC TROUBLESHOOTING COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the M-MDS. (See AFTER REPAIR PROCEDURE [L8, LF].) • Perform the Drive Mode 01 (Adopted Memory Procedure) and Drive Mode 03 (A/F sensor heater, HO2S heater, A/F sensor, HO2S and TWC Repair Verification). (See OBD DRIVE MODE [L8, LF].) • Is the PENDING CODE for this DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L8, LF].)
No | Go to the next step.
14 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [L8, LF].) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [L8, LF].)
No | DTC troubleshooting completed.