EMISSION SYSTEM LOCATION INDEX [L8, LF]

id0116a3803700

Engine Compartment Side

Except 6MT

amxzzw00000842

6MT

amxzzw00000843

1 | Quick release connector (See QUICK RELEASE CONNECTOR (EMISSION SYSTEM) REMOVAL/INSTALLATION [L8, LF].)
2 | PCV valve (See POSITIVE CRANKCASE VENTILATION (PCV) VALVE REMOVAL/INSTALLATION [L8, LF].) (See POSITIVE CRANKCASE VENTILATION (PCV) VALVE INSPECTION [L8, LF].)
3 | EGR valve (See EGR VALVE REMOVAL/INSTALLATION [L8, LF].) (See EGR VALVE INSPECTION [L8, LF].)
4 | Purge solenoid valve (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].) (See PURGE SOLENOID VALVE INSPECTION [L8, LF].)

Exhaust System Side

amxzzw00000844

1 | WU-TWC
2 | TWC

Fuel Tank Side

amxzzw00000845

1 | Fuel-filler cap
2 | Charcoal canister (See CHARCOAL CANISTER REMOVAL/INSTALLATION [L8, LF].) (See CHARCOAL CANISTER INSPECTION [L8, LF].)
3 | Evaporative chamber (See EVAPORATIVE CHAMBER REMOVAL/INSTALLATION [L8, LF].) (See EVAPORATIVE CHAMBER INSPECTION [L8, LF].)
4 | Rollover valve (See ROLLOVER VALVE REMOVAL/INSTALLATION [L8, LF].) (See ROLLOVER VALVE INSPECTION [L8, LF].)
5 | Check valve (two-way) (See CHECK VALVE (TWO-WAY) REMOVAL/INSTALLATION [L8, LF].) (See CHECK VALVE (TWO-WAY) INSPECTION [L8, LF].)