SELECTOR LEVER INSPECTION

id051400255500

1. Turn the ignition switch to the ON position (engine off).

2. With the brake pedal depressed, verify that there is a “click” at each range when shifted.

L.H.D.

amxzzw00000211

R.H.D.

amxzzw00000212

3. Verify that the selector lever can be shifted.

4. Verify that there is a “click” at each position when shifted from the P position to the M range.

5. Verify that the positions of the selector lever and the indicator are aligned.

amxzzw00000281

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT [SJ6A-EL].)

6. Verify that the vehicle operates in each selected range.