TCM REMOVAL/INSTALLATION [SJ6A-EL]

id051311250800

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

L.H.D.

amxzzw00000220

1 | TCM connector
2 | Nut
3 | Nut
4 | Bracket
5 | TCM

R.H.D.

amxzzw00000221

1 | TCM connector
2 | Nut
3 | Nut
4 | Bracket
5 | TCM