DECK PANEL MOTOR INSPECTION

id091600810200

1. Apply battery positive voltage and connect the ground to deck panel motor terminals A and E, and then inspect the deck panel motor operation.

e5e916zw6030

  • If the deck panel motor does not operate as indicated in the table, replace it.

  Caution
  • If the deck panel motor temperature is high, the motor may not rotate due to the motor internal PTC function. Leave it untouched for about 3 min to cool it down, then reinspect.

Operation | Terminal
--- | ---
E | A
Open | Ground | B+
Close | B+ | Ground

2. Connect the battery positive voltage to deck panel motor terminal D and connect terminal F to ground.

3. Operate the deck panel motor and measure the voltage at terminal B.

  • If there is any malfunction, replace the deck panel motor.

  Note
  • Terminal C is not used for the system control.

  Voltage

  • Pulse:max. 13 V/min. 0 V