CABIN TEMPERATURE SENSOR REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER]

id0740a1807800

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

L.H.D.

amxzzw00000697

R.H.D.

amxzzw00000698

1 | Air hose
2 | Cabin temperature sensor connector
3 | Cabin temperature sensor

5. Install in the reverse order of removal.