PARKING LIGHT BULB REMOVAL/INSTALLATION

id091800464900

LH

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the clip shown in the position in the figure.

amxzzw00001465

4. Set the wiring harness out of the way to ensure an operation space for the parking light removal.

5. Remove the socket, then remove the parking light bulb.

amxzzw00002029

6. Install in the reverse order of removal.

RH

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the nuts shown in the position in the figure.

amxzzw00001881

4. Set the coolant reserve tank out of the way to ensure an operation space for the parking light removal.

amxzzw00001467

5. Remove the socket, then remove the parking light bulb.

amxzzw00002030

6. Install in the reverse order of removal.