CLUTCH DRUM COMPONENT AND F4 ONE-WAY CLUTCH COMPONENT ASSEMBLY

id051300260800

Components

bsj6za00000622

1 | Bearing race
2 | Thrust needle spring
3 | Seal ring
4 | Input shaft component
5 | O-ring
6 | C1 clutch position
7 | C4 clutch position
8 | Piston return spring
9 | O-ring
10 | C1 clutch seal plate
11 | Snap ring
12 | Driven plate
13 | Drive plate
14 | Retaining plate
15 | Snap ring
16 | Driven plate
17 | Driven plate
18 | Drive plate
19 | Retaining plate
20 | Snap ring
21 | Bearing race
22 | Thrust needle bearing
23 | Clutch hub
24 | Thrust washer
25 | F4 one-way clutch

bsj6za00000623

1 | Snap ring
2 | C3 clutch seal plate
3 | Piston return spring
4 | O-ring
5 | C3 clutch piston component
6 | O-ring
7 | C2, C3 clutch drum
8 | O-ring
9 | C2 clutch piston
10 | C2 clutch piston return spring
11 | O-ring
12 | C2 clutch seal plate
13 | Snap ring
14 | Driven plate
15 | Drive plate
16 | Retaining plate
17 | Snap ring
18 | Snap ring
19 | Bearing race
20 | Thrust bearing
21 | Thrust washer
22 | Clutch hub
23 | Retaining plate
24 | Thrust needle bearing
25 | Clutch hub component
26 | Drive plate
27 | Driven plate
28 | Retaining plate
29 | Driven plate
30 | Sleeve
31 | Snap ring

Assembly Procedure

1. Apply ATF to the new O-rings.

2. Install the O-rings to the C2, C3 clutch drum.

bsj6za00000243

3. Apply ATF to the new O-rings.

4. Install the O-rings to the C3 clutch piston component.

bsj6za00000559

5. Apply ATF to the C2, C3 clutch drum and the C3 clutch piston component.

  Caution
  • Do not damage the O-ring.

6. Install the C2, C3 clutch drum to the C3 clutch piston component.

bsj6za00000883

7. Apply ATF to the seal plate and the piston return spring.

  Caution
  • Do not damage the O-ring.

8. Install the seal plate and the piston return spring to the C3 clutch hub component.

bsj6za00000561

9. Install the SST using a M10-1.25 bolt with a length of 100 mm as shown in the figure to compress the piston return spring.

bsj6za00000815

  Caution
  • Do not expand the snap ring too much.

10. Remove the snap ring using snap ring pliers.

bsj6za00000789

11. Apply ATF to the new O-rings.

12. Install the O-rings to the C2 clutch piston.

bsj6za00000562

13. Apply ATF to the new O-rings.

14. Install the O-rings to the C2 clutch seal plate.

bsj6za00000181

15. Apply ATF to the C2 clutch piston and the C2, C3 clutch drum.

  Caution
  • Do not damage the O-ring.

16. Install the C2 clutch piston and the C2, C3 clutch drum.

bsj6za00000563

17. Apply ATF to the C2 clutch seal plate and the C2, C3 clutch drum.

18. Install the C2 clutch seal plate and the C2 clutch piston return spring to the C2, C3 clutch drum.

bsj6za00000566

19. Install the SST as shown in the figure, and compress the C2 clutch piston return spring.

bsj6za00000875

  Caution
  • Do not expand the snap ring too much.

20. Install the snap ring using snap ring pliers.

bsj6za00000787

21. Apply ATF to the driven plate (C2) and the drive plate (C2) and the retaining plate (C2).

22. Install the driven plate (C2), the drive plate (C2), the retaining plate (C2) to the C2, C3 clutch drum.

bsj6za00000673

  Caution
  • Inspect the number of drive and driven plates.

23. Using a flathead screwdriver, install the snap ring (C2) to the C2, C3 clutch drum.

bsj6za00000186

  Caution
  • When installing the snap ring, set the end gap of the snap ring as shown in the figure.

24. Measure the retaining plate travel distance at both ends across the diameter using a dial gauge while blowing compressed air into the oil passage as shown in the figure, and calculate the average value. Verify that the piston moves smoothly.

bsj6za00000884

  Air pressure

  200 kPa (2 kgf/cm2, 28 psi)

Identification mark | Thickness (mm {in})
--- | ---
0 | 2.95—3.05 {0.016—0.120}
1 | 3.05—3.15 {0.120—0.124}
2 | 3.15—3.25 {0.124—0.128}
3 | 3.25—3.35 {0.128—0.132}
4 | 3.35—3.45 {0.132—0.136}
5 | 3.45—3.55 {0.136—0.140}
6 | 3.55—3.65 {0.140—0.144}
7 | 3.65—3.75 {0.144—0.148}
8 | 3.75—3.85 {0.148—0.152}

  Caution
  • If the C2 clutch pack clearance exceeds the maximum specification, select another retaining plate.

25. Using a flathead screwdriver, install the snap ring (C3) to the C2, C3 clutch drum.

bsj6za00000188

  Caution
  • When installing the snap ring, set the end gap of the snap ring as shown in the figure.

26. Apply ATF to the retaining plate (C3), the driven plate (C3), the drive plate (C3).

  Caution
  • Inspect the number of drive and driven plates.

27. Install the retaining plate (C3) and the driven plate (C3) and the drive plate (C3) and the sleeve to the C2, C3 clutch drum.

bsj6za00000674

  Caution
  • When installing the snap ring, set the end gap of the snap ring as shown in the figure.

28. Using a flathead screwdriver, install the snap ring (C3) to the C2, C3 clutch drum.

bsj6za00000190

29. Measure the driven plate travel distance of the reverse piston travel distance and driven plate at the both ends across the diameter using a dial gauge while blowing compressed air into the oil passage as shown in the figure, and calculate the average value. Verify that the piston moves smoothly.

bsj6za00000885

  Air pressure

  200 kPa (2 kgf/cm2, 28 psi)

  Standard travel distance A

  1.62—2.68 mm {0.06—0.10 in}

  Standard travel distance B

  1.22—1.67 mm {0.05—0.06 in}

  Standard gap

  0.40—0.70 mm {0.01—0.03 in}

Identification mark | Thickness (mm {in})
--- | ---
0 | 2.35—2.45 {0.093—0.096}
1 | 2.45—2.55 {0.096—0.100}
2 | 2.55—2.65 {0.100—0.104}
3 | 2.65—2.75 {0.104—0.108}
4 | 2.75—2.85 {0.108—0.112}
5 | 2.85—2.95 {0.112—0.116}
6 | 2.95—3.05 {0.116—0.120}
7 | 3.05—3.15 {0.120—0.124}
8 | 3.15—3.25 {0.124—0.128}
9 | 3.25—3.35 {0.128—0.132}
A | 3.35—3.45 {0.132—0.136}
B | 3.45—3.55 {0.136—0.140}

  Caution
  • If the C3 clutch pack clearance exceeds the maximum specification, select another retaining plate.

30. Apply ATF to the sliding surface of the new seal ring input shaft.

  Caution
  • Do not expand the seal ring too much.
  • Be careful not to shorten the seal rings too much, when installing them.

31. Compress the seal rings as shown in the figure and install them to the input shaft component.

bsj6za00000675

  Note
  • Verify that oil seal rings rotate smoothly after installing them.

32. Apply ATF to the new D-ring.

33. Install the D-ring to the C4 clutch seal plate.

bsj6za00000567

34. Apply ATF to the new O-ring.

35. Install the O-ring to the input shaft component.

bsj6za00000568

36. Apply ATF to the C1 clutch piston and the C4 clutch piston to the input shaft component.

37. Install the C1 clutch piston and the C4 clutch piston to the input shaft component.

bsj6za00000569

38. Apply ATF to the C1 clutch seal plate and the input shaft component.

39. Install the C1 clutch seal plate and the piston return spring to the input shaft component.

bsj6za00000676

  Caution
  • Do not damage the D-ring.

40. Place the SST on the C1 clutch seal plate and compress the piston return spring with a press.

  Caution
  • Do not expand the snap ring too much.

41. Install the snap ring using snap ring pliers.

bsj6za00000871

42. Apply ATF to the retaining plate (C4), the driven plate (C4), the drive plate (C4).

  Caution
  • Inspect the number of drive and driven plates.

43. Install the retaining plate (C4), the driven plate (C4), the drive plate (C4) to the input shaft component.

bsj6za00000677

44. Using a flathead screwdriver, install the snap ring to the input shaft component.

bsj6za00000199

45. Measure the retaining plate travel distance at both ends across the diameter using a dial gauge while blowing compressed air into the oil passage as shown in the figure, and calculate the average value. Verify that the piston moves smoothly.

bsj6za00000886

  Air pressure

  200 kPa (2 kgf/cm2, 28 psi)

  Standard travel distance

  0.02—1.01 mm {0.0008—0.0397 in}

  Standard gap

  0.4—0.7 mm {0.0158—0.0275 in}

Identification mark | Thickness (mm {in})
--- | ---
0 | 2.95—3.05 {0.116—0.120}
1 | 3.05—3.15 {0.120—0.124}
2 | 3.15—3.25 {0.124—0.128}
3 | 3.25—3.35 {0.128—0.132}
4 | 3.35—3.45 {0.132—0.136}
5 | 3.45—3.55 {0.136—0.140}
6 | 3.55—3.65 {0.140—0.144}
7 | 3.65—3.75 {0.144—0.148}
8 | 3.75—3.85 {0.148—0.152}
9 | 3.85—3.95 {0.152—0.156}

  Caution
  • If the C4 clutch pack clearance exceedy the maximum specification, select another retaining plate.

46. Apply ATF to the retaining plate (C1), the driven plate (C1), the drive plate (C1).

  Caution
  • Inspect the number of drive and driven plates.

47. Install the retaining plate (C1), the driven plate (C1), the drive plate (C1) to the input shaft component.

bsj6za00000678

48. Using a flathead screwdriver, install the snap ring to the input shaft component.

bsj6za00000202

49. Measure the retaining plate travel distance at both ends across the diameter using a dial gauge while blowing compressed air into the oil passage as shown in the figure, and calculate the average value. Verify that the piston moves smoothly.

bsj6za00000887

  Air pressure

  200 kPa (2 kgf/cm2, 28 psi)

  Standard travel distance

  0.14—0.17 mm {0.0056—0.0066 in}

  Standard gap

  0.56—0.86 mm {0.0221—0.0338 in}

  Caution
  • If the C1 clutch pack clearance exceedy the maximum specification, select another retaining plate.

50. Apply ATF to the F4 one-way clutch and the thrust washer.

51. Install the F4 one-way clutch to the clutch hub.

bsj6za00000204

52. Apply ATF to the bearing race.

53. Install the bearing race to the C1, C4 clutch component.

bsj6za00000205

54. Install the clutch hub to the C1, C4 clutch component.

bsj6za00000679

55. Apply ATF to the bearing race.

56. Install the bearing race to the C3 clutch piston component.

bsj6za00000207

57. Install the C1, C4 clutch component to the C2, C3 clutch drum.

bsj6za00000594

58. Apply ATF to the thrust bearing, the bearing race and the thrust washer.

59. Install the thrust bearing, bearing race and thrust washer.

bsj6za00000209

60. Install the clutch hub to the C3 clutch piston component.

bsj6za00000818

61. Apply ATF to the thrust needle spring.

62. Install the thrust needle spring to the clutch hub.

bsj6za00000211

63. Apply ATF to the retaining plate.

64. Install the retaining plate to the C3 clutch piston component.

bsj6za00000571

65. Install the clutch hub component to the C3 clutch piston component.

bsj6za00000819

66. Apply ATF to the retaining plate, the drive plate, the driven plate.

  Caution
  • Inspect the number of drive and driven plates.

67. Install the retaining plate (C3), the drive plate (C3), and the driven plate (C3) to the clutch hub component.

bsj6za00000682

68. Using a flathead screwdriver, install the snap ring to the C3 clutch piston component.

bsj6za00000820