HEADLIGHT CLEANER HOSE REMOVAL/INSTALLATION

id091900803100

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Disconnect joint pipe.

amxzzw00001190

5. Disconnect headlight cleaner hose from the headlight cleaner actuator.

6. Remove the headlight cleaner hose from the front bumper.

7. Install in the reverse order of removal.