CYLINDER HEAD DISASSEMBLY (II)

id011000500500

1. Disassemble in the order indicated in the table.

belbze00000048

1 | Engine hanger
2 | Valve keeper (See Valve Keeper Disassembly Note.)
3 | Upper valve spring seat
4 | Valve spring
5 | Valve
6 | Valve seal (See Valve Seal Disassembly Note.)
7 | EGR pipe
8 | Water outlet case

Valve Keeper Disassembly Note

1. Remove the valve keeper using the SSTs.

When using the SSTs (49 0636 100B, 49 B012 0A2)

belbze00000049

When using the SST (49 JE02 0A2) (Europe only)

belbze00000050

Valve Seal Disassembly Note

1. Remove the valve seal using the SST.

belbze00000051