DTC B1011:95 [ACTIVE BONNET]

id0802f1823100

DESCRIPTION | Active bonnet control module connector partially disconnected
--- | ---
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the diagnostic procedure. • No continuity between partially disconnected detector bar terminals of active bonnet control module
POSSIBLE CAUSE | • Active bonnet control module connector partially disconnected • Active bonnet control module connector malfunction • Active bonnet control module malfunction
SYSTEM WIRING DIAGRAM |

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | INSPECT CONNECTION CONDITION OF ACTIVE BONNET CONTROL MODULE Warning • Handling the component parts improperly can accidentally operate the active bonnet actuator, which may seriously injure you. Read the service warnings and cautions before handling the component parts of the active bonnet. (See ACTIVE BONNET SERVICE WARNINGS.) (See ACTIVE BONNET SERVICE CAUTIONS.) • Switch the ignition to LOCK. • Disconnect the negative battery cable and wait 1 min or more. • Disconnect the active bonnet actuator (RH, LH) connector. • Remove the partition board. (See PARTITION BOARD REMOVAL/INSTALLATION.) • Remove the trunk side trim (RH). (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.) • Are all active bonnet control module connectors correctly connected? | Yes | Go to the next step.
No | Connect the active bonnet control module connector correctly. Go to Step 3.
2 | VERIFY PARTIALLY DISCONNECTED TERMINAL BAR OF ACTIVE BONNET CONTROL MODULE • Disconnect the active bonnet control module connector. (See ACTIVE BONNET CONTROL MODULE REMOVAL/INSTALLATION.) • Verify the condition of the partially disconnected terminal bar (vehicle wiring harness side) of the active bonnet control module. (Corrosion, damage, and disconnected pins) • Is the partially disconnected terminal bar of the active control module normal? | Yes | Go to the next step.
No | Replace the wiring harness, then go to the next step.
3 | PERFORM DTC INSPECTION FOR ACTIVE BONNET CONTROL MODULE • Connect the active bonnet control module connector. • Reconnect all the disconnected connectors. • Connect the negative battery cable. • Switch the ignition ON. • Clear the DTC for the active bonnet control module using the M-MDS. (See CLEARING DTC [ACTIVE BONNET].) • Perform the active bonnet control module DTC inspection using the M-MDS. (See DTC INSPECTION [ACTIVE BONNET].) • Is the same DTC displayed? | Yes | Replace the active bonnet control module. (See ACTIVE BONNET CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.