DTC B2477 [INSTRUMENT CLUSTER]

id0902e8352800

DTC B2477 | • Instrument cluster configuration not performed
--- | ---
DETECTION CONDITION | • Configuration write failure is detected. (i.e. instrument cluster is replaced)
POSSIBLE CAUSE | • Configuration procedure has not been performed. • Instrument cluster malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | PERFORM INSTRUMENT CLUSTER CONFIGURATION • Perform instrument cluster configuration. • Is B2477 displayed? | Yes | Replace the instrument cluster.
No | Go to the next step.
2 | VERIFY TROUBLESHOOTING OF DTC B2477 COMPLETED • Clear the DTC from the memory. • Is B2477 displayed? | Yes | Go to the applicable DTC inspection.
No | DTC troubleshooting completed.