NO.1 CD PLAYER/CHANGER DOES NOT LOAD THE CD OR EJECTS THE CD IMMEDIATELY [CD PLAYER/CHANGER]

id0903e5826100

1 | CD player/changer does not load the CD or ejects the CD immediately
--- | ---
Possible DTC | 10:Er01, 22:Er01
POSSIBLE CAUSE | • CD is inserted upside down • Defective CD (e.g., cracked, badly bent, rough edges, scratch, dirty CD, condensation) • Non-conventional discs (e.g., 8 cm (3 in) CD, 8 cm (3 in) disc adapter, heart-shaped disc, octagonal disc) • Deformed disc is used (e.g., out of specification (thickness), bent disc) • Poor connection of center panel unit connector or terminal (e.g., damaged, bent, pulled-out pin, corrosion) • Audio unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is CD inserted properly, label-side up? | Yes | Go to the next step.
No | Explain to the customer that CD should be inserted into the slot, label-side up.
2 | • Replace with a CD known to be good. • Does the CD player/changer load the CD? | Yes | Go to the next step.
No | Replace the audio unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION). (See CENTER PANEL UNIT DISASSEMBLY/ASSEMBLY).
3 | • Visually inspect the CD. ― Is there any dirt, scratch or deformation on the CD? ― Is the CD a non-conventional disc? | Yes | Explain to the customer that the defective CD or non-conventional disc cannot be use.
No | Go to the next step.
4 | • Turn the ignition switch to the LOCK position. • Inspect the connection of the audio unit connector (24-pin). • Inspect both audio unit connector and wiring harness-side connector for poor connection. (such as damaged/bent/pulled-out pins, corrosion) • All the pins and connector normal? | Yes | Replace the audio unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION). (See CENTER PANEL UNIT DISASSEMBLY/ASSEMBLY).
No | If the audio unit connector/pin is wrong: • Replace the audio unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION). (See CENTER PANEL UNIT DISASSEMBLY/ASSEMBLY). If the wiring harness-side connector/pin is wrong: • Repair or replace the pins and/or the connector.