ENGINE DISASSEMBLY/ASSEMBLY [L8, LF]

id0110a9800500

1. Remove the transmission from the engine. (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].)(See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].) (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION [SJ6A-EL].)

2. Remove the following parts:

  (1) The clutch unit (MT) (See CLUTCH UNIT REMOVAL/INSTALLATION.)

  (2) The ignition coil (See IGNITION COIL REMOVAL/INSTALLATION [L8, LF].)

  (3) The CMP sensor (See CAMSHAFT POSITION (CMP) SENSOR REMOVAL/INSTALLATION [L8, LF].)

  (4) The power steering oil pump (See POWER STEERING OIL PUMP REMOVAL/INSTALLATION.)

  (5) The fuel distributor and fuel injector (See FUEL INJECTOR REMOVAL/INSTALLATION [L8, LF].)

  (6) The intake-air system (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)

  (7) The exhaust system (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

  (8) The CKP sensor (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [L8, LF].)

3. Remove the drive belt auto tensioner .

amxzzw00002160

4. Install in the reverse order of removal.