OIL SEAL (EXTENSION HOUSING) REPLACEMENT [SJ6A-EL]

id051311710000

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Clean the transmission exterior thoroughly using a steam cleaner or cleaning solvent.

4. Drain the ATF. (See AUTOMATIC TRANSMISSION FLUID (ATF) REPLACEMENT [SJ6A-EL].)

5. Remove the following parts.

  (1) Tunnel member component

  (2) Middle pipe (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

  (3) Power plant frame (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION [SJ6A-EL].)

  (4) Propeller shaft (See PROPELLER SHAFT REMOVAL/INSTALLATION.)
    Caution
    • Do not to damage the extension dust deflector.
    • Do not to damage the extension housing.

6. Using a plastic hammer and slab of wood, tap the extension dust deflector to remove it.

ar8jjw00001011

7. Using a tape-wrapped flathead screwdriver, remove the extension housing shroud.

ar8jjw00001012

8. Using a tape-wrapped flathead screwdriver, remove the oil seal.

ar8jjw00001013

9. Using the SST and a hammer, install the new oil seal to the extension housing.

e5u513zw5044

10. Coat the oil seal lip with grease.

11. Using the SST and a hammer, install the new extension housing shroud to the extension housing.

e5u513zw5043

12. Using a hammer and slab of wood, install the extension dust deflector to the extension housing.

13. Install the following parts.

  (1) Propeller shaft (See PROPELLER SHAFT REMOVAL/INSTALLATION.)

  (2) Power plant frame (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION [SJ6A-EL].)

  (3) Middle pipe (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

  (4) Tunnel member component

14. Add ATF and, with the engine idling, inspect the ATF level and for leakage. (See AUTOMATIC TRANSMISSION FLUID (ATF) LEVEL ADJUSTMENT [SJ6A-EL].)

15. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

16. Install the battery cover.