BRAKE SPECIFICATIONS

id040000100300

Item | Specification
--- | ---
Brake pedal | Type | Suspended design
Pedal lever ratio | 2.9
Max. stroke | (mm {in}) | 133 {5.24}
Master cylinder | Type | Tandem (plunger type)
Cylinder bore | (mm {in}) | 22.2 {0.87}
Front brake (disc) | Type | Ventilated disc
Cylinder bore | (mm {in}) | 54.0 {2.13}
Pad dimensions (area x thickness) | 4,670 x 9 {7.472 x 0.35}
(mm2 x mm {in2 x in})
Disc plate dimensions (outer diameter x thickness) | 290 x 22 {11.4 x 0.87}
(mm {in})
Rear brake (disc) | Type | Solid disc
Cylinder bore | (mm {in}) | 38.18 {1.5}
Pad dimensions (area x thickness) | 2,470 x 7.5 {3.952 x 0.3}
(mm2 x mm {in2 x in})
Disc plate dimensions (outer diameter x thickness) | 280 x 10 {11.0 x 0.39}
(mm {in})
Power brake unit | Type | Vacuum multiplier Single diaphragm
Outer diameter | (mm {in}) | 248 {9.75}
Rear wheel braking force control device | Type | EBD (Electronic brakeforce distribution)
Parking brake | Type | Mechanical two-rear-wheel control
Operation system | Center lever type
Brake fluid | Type | European (L.H.D. U.K.) specs.: SAE J1703, FMVSS 116 DOT-3 or DOT-4 Australian, General (L.H.D.) specs.: SAE J1703, FMVSS 116 DOT-3