THROTTLE POSITION (TP) SENSOR INSPECTION [L8, LF]

id0140i7802700

  Caution
  • This inspection procedure cannot be completed correctly if the accelerator pedal position sensor has a malfunction. Before performing this procedure, verify that any one of the DTCs related to the accelerator pedal position sensor is not detected.

1. Verify that no DTC related to APP sensor has been detected.

  • If any DTCs related to APP sensor have been detected, perform the DTC inspection. (See DTC TABLE [L8, LF].)

2. Connect the M-MDS to the DLC‐2.

amxzzw00000041

3. Turn the ignition switch to the ON position.

4. Select TP1 or TP2 PID (percentage) on the M-MDS.

5. Verify that the TP sensor output voltage (M-MDS PID: TP1, TP2) is within the specification. (See PCM INSPECTION [L8, LF].)

• If not as specified, replace the throttle body. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)