DOOR MODULE PANEL REMOVAL/INSTALLATION

id091100602600

1. Disconnect the negative battery cable.(See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Door trim (See DOOR TRIM REMOVAL/INSTALLATION.)

  (2) Door speaker (See DOOR SPEAKER REMOVAL/INSTALLATION.)

3. Disconnect the power outer mirror harness connector.

4. Disconnect the door lock actuator connector.

5. Disconnect the power window motor connector.

6. Remove screws A and B.

amxzzw00002141

7. pull the door module panel outward and detach clips C.

8. Remove the door module panel.

9. Install in the reverse order of removal.