KNOCK SENSOR (KS) INSPECTION [L8, LF]

id0140i7802800

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the KS connector.

4. Measure resistance between KS terminals A and B.

  • If not within the specification, replace the KS. (See KNOCK SENSOR (KS) REMOVAL/INSTALLATION [L8, LF].)

  KS Specification

  Approx. 4.87 megohms [normal temperature]