CLEARING DTC [HANDS-FREE TELEPHONE (HF/TEL) SYSTEM]

id0902g0400300

  Caution
  • Before clearing the memory, be sure to enter all of the DTCs displayed in the on-board diagnostic test mode in the Audio Repair Order Form.

1. Launch the on-board diagnostic test mode. (See STARTING PROCEDURE FOR ON-BOARD DIAGNOSTIC TEST MODE [HANDS-FREE TELEPHONE (HF/TEL) SYSTEM].)

2. While pressing the AUTO-M switch, simultaneously press the RPT/PRESET switch 4 for 2 s or more.

amxzzw00000966

3. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.