BACK-UP LIGHT SWITCH REMOVAL/INSTALLATION [M15M-D]

id051110248000

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the back-up light switch connector and remove the back-up light switch.

amxzzw00001877

4. Install the back-up light switch (with a new gasket) to the transaxle case.

  Tightening torque

  25—34 N·m {2.5—3.5 kgf·m, 18—25 ft·lbf}

5. Install in the reverse order of removal.