ACTIVE BONNET WARNING ALARM CONSTRUCTION/OPERATION

id081300002800

• The active bonnet warning alarm sounds from a buzzer in the instrument cluster.

amxzzn00000697

• The active bonnet control module sends the active bonnet warning alarm trigger signal to the instrument cluster via CAN communication to sound the buzzer in the instrument cluster.
• If the active bonnet control module detects DTC B00D2:01 and DTCs other than B00D2:01 (except for active bonnet warning light is not illuminated DTCs), an active bonnet warning alarm sound trigger signal is sent to the instrument cluster.

  Note
  • DTC B00D2:01 (Active bonnet warning light malfunction)

amxzzn00000698

• Refer to the instrumentation/driver information specifications for the active bonnet warning alarm sound interval. (See INSTRUMENT CLUSTER SPECIFICATIONS.)