SEAT BACK TRIM REMOVAL/INSTALLATION

id091300987100

L.H.D.

1. Turn the ignition switch to LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the screw, then remove the belt guide.

amxzzw00001603

5. Slide hook A in the direction of arrow (1), (2), (3) shown in the figure to detach it from hook B.

amxzzw00001597

6. Open the fastener.

amxzzw00001598

7. Remove ring C, then remove the holder bracket C in the direction of arrow.

amxzzw00001599

8. Pull out part A shown in the figure to the front.

amxzzw00001600

9. Disconnect the seat warmer connector.

10. Remove the seat back trim and the seat back pad as a single unit from the seat frame by pulling them in the direction of arrow.

amxzzw00001601

11. Partially peal back the seat back trim from the seat back pad, remove rings C in the order of (4), (5), (6) and (7) shown in the figure, then remove the seat back trim.

amxzzw00002175

12. Install in the reverse order of removal.

R.H.D.

1. Turn the ignition switch to LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the screw, then remove the belt guide.

amxzzw00001596

5. Slide hook A in the direction of arrow (1), (2), (3) shown in the figure to detach it from hook B.

amxzzw00001604

6. Open the fastener.

amxzzw00001605

7. Remove ring C, then remove the holder bracket C in the direction of arrow.

amxzzw00001606

8. Pull out part A shown in the figure to the front.

amxzzw00001870

9. Disconnect the seat warmer connector.

10. Remove the seat back trim and the seat back pad as a single unit from the seat frame by pulling them in the direction of arrow.

amxzzw00001871

11. Partially peal back the seat back trim from the seat back pad, remove rings C in the order of (4), (5), (6) and (7) shown in the figure, then remove the seat back trim.

amxzzw00002176

12. Install in the reverse order of removal.