STEERING ANGLE SENSOR FUNCTION

id041500102400

• The steering angle sensor, located on the combination switch, detects the steering angle degree and the neutral position, and transmits these to the DSC HU/CM via CAN lines.

  Warning
  • The following circumstances will cause the stored initialization value of the steering angle sensor to be cleared. This may possibly cause an accident due to the DSC becoming inoperative. Always refer to the Workshop Manual and properly perform the initialization procedure for the steering angle sensor so that the DSC operates properly.
    ― Negative battery cable disconnection
    ― Steering angle sensor connector disconnection
    ― Fuse (ROOM 15A) removal
    ― Wiring harness disconnection between battery and steering angle sensor connector

  Note
  • If the initialization procedure for the steering angle sensor has not been performed, when the ignition switch is turned to the ON position, the DSC indicator light illuminates and the DSC OFF light flashes to warn of a malfunction.