THROTTLE BODY INSPECTION [L8, LF]

id0113a3802600

Resistance Inspection

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the throttle body connector.

4. Measure the resistance between throttle actuator terminals A and B.

amxzzw00000799

  Throttle body resistance

  0.3—100 ohms [20 °C {68 °F}]

  • If not as specified, replace the throttle body. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)