BONNET STRIKER REMOVAL/INSTALLATION

id091400800300

  Warning
  • After the active bonnet has deployed, always newly replace the parts indicated in the active bonnet service warnings in the section dealing with the active bonnet. If the vehicle is driven without part replacement, the active bonnet may not deploy correctly. (See ACTIVE BONNET SERVICE WARNINGS.)

1. Remove the bolt, then remove the bonnet striker.

amxzzw00002750

2. Install in the reverse order of removal.