DOOR SPEAKER REMOVAL/INSTALLATION

id092000807200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the door trim.(See DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

amxzzw00002306

1 | Screw
2 | Door speaker (See Door Speaker Installation Note.)
3 | Connector

5. Install in the reverse order of removal.

Door Speaker Installation Note

  Caution
  • If the speaker is installed with the wiring harness out of the groove, an open circuit in the wiring harness could occur.

1. Remove the speaker with the wiring harness passing through the groove of the door module.

amxzzw00002187