DOOR SPEAKER INSPECTION

id092000806900

1. Verify the resistance between door speaker terminals.

amxzzw00001679

  • If the resistance is not within the specification, replace the door speaker.

  Resistance

  Without Bose®: 4 ohm
  With Bose®: 1 ohm

2. Connect a 1.5 V battery to the door speaker and verify that noise is heard from the door speaker.

  • If no noise is heard, replace the door speaker.